;
; Generated file, do not edit
;
; Copyright (c) 1998-2001 Fuji Xerox
; 
;
[Version]
Signature="$Windows NT$"
Provider=%OEM%
LayoutFile=FXXLLSTI.inf
ClassGUID={4D36E979-E325-11CE-BFC1-08002BE10318}
Class=Printer
DriverVer=03/06/2002

;
; The Manufacturer section lists all of the manufacturers that we will
; display in the Dialog box
;

[Manufacturer]
"Fuji Xerox"

;
; Model sections. Each section here corresponds with an entry listed in the
; [Manufacturer] section, above. The models will be displayed in the order
; that they appear in the INF file.
;

[Fuji Xerox]
"Xerox DC 400/350/250 PCL 6 (T)" = DC406T,

;
; Installer Sections
;
; These sections control file installation, and reference all files that
; need to be copied. The section name will be assumed to be the driver
; file, unless there is an explicit DriverFile section listed.
;

[DC406T]
CopyFiles=DC406T_DLL,DC406T_HLP,DC406TADC
DataSection=DC406T_DATA
DataFile=DC406TK.DLL

; Copy Sections
;
; Lists of files that are actually copied. These sections are referenced
; from the installer sections, above. Only create a section if it contains
; two or more files (if we only copy a single file, identify it in the
; installer section, using the @filename notation) or if it's a color
; profile (since the DestinationDirs can only handle sections, and not
; individual files).
;

[DC406T_DLL]
DC406TK.DLL
DC406TU.DLL
DC406TP.DLL
DC406TC.DLL
DC406TL.DLL
DC406TX.DLL
DC406TS.DLL
DC406TJ.DLL
DC406TQ.EXE
DC406TWU.DLL
DC406TWK.DLL
DC406TZU.DLL
DC406TZK.DLL
DC406TZ1.EXE

[DC406T_HLP]
DC406T.HLP

[DC406TADC]
FXZADCT.EXE
pmaMIB.dll
pmaUtil.dll
PmcAsn.dll
pmcComn.dll
pmcComnF.dll
pmcLog.dll
pmcSock.dll
pmfComn.dll
pmfSMB.dll
pmfSNMP.dll
pmmDev.dll
pmmPIMgr.dll
pmsSnmp.dll
pmtTrap.dll
pmuFiltr.dll
pmuNet.dll
pswCIF.dll
pswComn.dll
pswFXLeg.dll
pswXCMI.dll
addreso.dll
pmaIETF.xmm
pmaFXLeg.xmm
pmaXCMI.xmm
pmaXJob.xmm
psw550AP.xpi
pswLegAP.xpi
psw750AP.xpi
psw285AP.xpi

;
; Data Sections
;
; These sections contain data that is shared between devices.
;
[DC406T_DATA]
DriverFile=DC406TK.DLL
ConfigFile=DC406TU.DLL
HelpFile=DC406T.HLP
;
; diskid = description,tagfile,unused,subdir
;
[SourceDisksNames]
1 = %DISKDESC% ,,,""

;
; filename_on_source = diskid,subdir,size,checksum,spare,spare
; extra fields are nt-specific
;   bootmediaord,targetdirectory,upgradedisposition,textmodedisposition,targetname
;
[SourceDisksFiles]
DC406TZ1.EXE=1
DC406TK.DLL=1
DC406TU.DLL=1
DC406TL.DLL=1
DC406TP.DLL=1
DC406TC.DLL=1
DC406TJ.DLL=1
DC406TQ.EXE=1
DC406TX.DLL=1
DC406TS.DLL=1
DC406TWU.DLL=1
DC406TWK.DLL=1
DC406TZU.DLL=1
DC406TZK.DLL=1
DC406T.HLP=1
FXZADCT.EXE=1
pmaMIB.dll=1
pmaUtil.dll=1
PmcAsn.dll=1
pmcComn.dll=1
pmcComnF.dll=1
pmcLog.dll=1
pmcSock.dll=1
pmfComn.dll=1
pmfSMB.dll=1
pmfSNMP.dll=1
pmmDev.dll=1
pmmPIMgr.dll=1
pmsSnmp.dll=1
pmtTrap.dll=1
pmuFiltr.dll=1
pmuNet.dll=1
pswCIF.dll=1
pswComn.dll=1
pswFXLeg.dll=1
pswXCMI.dll=1
addreso.dll=1
pmaIETF.xmm=1
pmaFXLeg.xmm=1
pmaXCMI.xmm=1
pmaXJob.xmm=1
psw550AP.xpi=1
pswLegAP.xpi=1
psw750AP.xpi=1
psw285AP.xpi=1

;
; Call SetupSetDirectoryId with 66000 to set the target directory at runtime
; (depending on which environment drivers are getting installed)
;

[DestinationDirs]
DefaultDestDir=66000


;
; Localizable Strings
;
[Strings]
OEM="Fuji Xerox"
DISKDESC="Xerox DC 400/350/250 PCL 6 (T)"
